[***  Modification in I-7565-H1/H2_Utility_v1.17  ***] (2016/10/27)
1. Solve the "CANData Message Display" problem when RTR=1 in "OverWrite" and "Record" mode.


[***  Modification in I-7565-H1/H2_Utility_v1.16  ***] (2016/07/21)
1. In "OverWrite" mode, add the Max/Min time interval of CAN message in "CycleTime" field.
2. Solve the "Load File Format Error" problem.
3. Improve "Load Configuration" function.
4. Add "I-7565-H1H2_Utility_Win10.exe" for Windows 10 platform


[***  Modification in I-7565-H1/H2_Utility_v1.15  ***]
1. Add "Total Column" in "OverWrite" Mode.
2. Solve the frozen TimeStamp problem.


[***  Modification in I-7565-H1/H2_Utility_v1.14  ***]
1. Modify "Save Reception List" Function in "OverWrite" Mode.


[***  Modification in I-7565-H1/H2_Utility_v1.13  ***]
1. Add "Load Reception List" option in the menu of "File" item.


[***  Modification in I-7565-H1/H2_Utility_v1.12  ***]
1. Add "CAN Error Frame" information function in "CAN RecvMsg" field.
2. In "Advanced Config" screen, add below three options:
   (1) "Set CAN Error Frame Function" option => enable/disable CAN error frame function
   (2) "Get CAN Error Frame Function" option => get CAN error frame function enabled or not.
   (3) "Get CAN1/2 Baud Bit-Timing Parameter" => get CAN baud bit-timing parameter including Tseg1/Tseg2/SJW value.
3. Extend "User-Defined CAN Baud" function in connection screen, users can choose the different sample point of bit-time (Tseg2 Value) in the same CAN baud.


[***  Modification in I-7565-H1/H2_Utility_v1.11  ***]
1. Modify just Show ComPort No. of I-7565-H1/H2 module in "Com Port." combobox field of utility.


[***  Modification in I-7565-H1/H2_Utility_v1.10  ***]
1. Add "Arbitration Lost" error information in bit5 of CANReg field. (Supported in FW_v1.06 or newer)
2. Provide "CAN-ID Tagging" function (replace the CAN-ID by a symbolic name) in OverWrite Mode
3. Add "FrmInternal" screen and provide the flash data of CAN1/2 Filter-ID reset function for "could not set comm state" error when connecting to I-7565-H1/H2 via utility.


[***  Modification in I-7565-H1/H2_Utility_v1.09  ***]
1. Add "Listen Only Mode" Function
2. Increase HWSendTimer Number from 1 set to 5 sets and add "AddMode" and "AddVal" parameter for HW_SendTimer Function
3. Add Trend Screen of CANbus DataFlow Function
4. Add "Scroll" and "OverWrite" mode option for CAN RecvMsg Table


[***  Modification in I-7565-H1/H2_Utility_v1.08  ***]
1. Add "Hardware Serial Number" Function in module information


[***  Modification in I-7565-H1/H2_Utility_v1.06  ***]
1. Support to input decimal value in "Timer(ms)" field for "HWSend" button function. For example, if users input 0.5 in Timer field and click "HWSend" button. Then I-7565-H1/H2 will send CAN messages with 0.5ms period. The smalleset value in Timer field is 0.2. This function is supported with firmware version v1.03 or newer in I-7565-H1/H2 module.



